(footprint "WH148 1A 4" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at 0 2.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 516ec78d-aac6-4552-88e4-370b4cebf71d)
  )
  (fp_text value "WH148 1A 4" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1d8a6581-9f5b-4bdd-8601-550f4c327131)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 0a9700c3-9a9e-4f69-ba6f-99a8c70e6baf)
  )
  (fp_line (start 3.5 -5) (end 3.5 0) (layer "F.Fab") (width 0.1) (tstamp 24b8b4de-c97f-41e9-95ad-2f4cef71e20a))
  (fp_line (start -1.5 0) (end 1.5 0) (layer "F.Fab") (width 0.1) (tstamp 3c682a8a-dc41-4c3a-ad4f-b11011753261))
  (fp_line (start -1.5 -5) (end -1.5 0) (layer "F.Fab") (width 0.1) (tstamp 3ea101d9-13b5-4c07-b295-c65054b4fe04))
  (fp_line (start 7.5 -5) (end 7.5 -13.5) (layer "F.Fab") (width 0.1) (tstamp 5e85f21e-0bed-40b3-8ac2-271617ad732d))
  (fp_line (start 3.5 0) (end 6.5 0) (layer "F.Fab") (width 0.1) (tstamp 8984ce21-7313-4450-acec-a9f0115fdc16))
  (fp_line (start -6.5 0) (end -3.5 0) (layer "F.Fab") (width 0.1) (tstamp a5aa8575-b54b-42c5-af57-1f5e7d8104ef))
  (fp_line (start -3.5 0) (end -3.5 -5) (layer "F.Fab") (width 0.1) (tstamp c01e7458-bbc6-4d26-b302-8f4fbc4c311b))
  (fp_line (start -7.5 -5) (end 7.5 -5) (layer "F.Fab") (width 0.1) (tstamp d5a4c1ca-d9a0-439b-938f-74943f820bec))
  (fp_line (start 1.5 0) (end 1.5 -5) (layer "F.Fab") (width 0.1) (tstamp e3f6c3ba-010c-4649-bee8-c546bc5a1ed0))
  (fp_line (start -6.5 -5) (end -6.5 0) (layer "F.Fab") (width 0.1) (tstamp e6ff2da1-ad48-4cec-ae48-c4516945720d))
  (fp_line (start -7.5 -13.5) (end -7.5 -5) (layer "F.Fab") (width 0.1) (tstamp ef1a051b-cd25-44e9-9814-e719506163de))
  (fp_line (start 6.5 0) (end 6.5 -5) (layer "F.Fab") (width 0.1) (tstamp f1235e3c-9c28-4819-87d1-6460322d4be1))
  (fp_circle (center 0 -17.5) (end 0 -9) (layer "F.Fab") (width 0.1) (fill none) (tstamp 24da9890-98da-4b7f-b4ee-407d66e36baf))
  (fp_circle (center 0 -17.5) (end 0 -14.5) (layer "F.Fab") (width 0.1) (fill none) (tstamp 8188e069-4faf-4de5-87f5-28b7bfa64d78))
  (pad "1" thru_hole circle (at -5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask) (tstamp f87b284d-b0ff-48dc-a3c9-10bcd68de52b))
  (pad "2" thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask) (tstamp 2a79b452-37a8-4b88-af21-7f343fe2699d))
  (pad "3" thru_hole circle (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask) (tstamp b9f037da-fae0-418e-bb59-8b60572e1dfe))
  (model "/home/marble/wtf/2022019/Alternator_Motor_Driver/assets/3D models/WH148.step"
    (offset (xyz 0 -0.5 14))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
