** Drc report for /home/marble/wtf/2022019/ABS_Simulator_Panel/source/ABS_Simulator_Panel.kicad_pcb **
** Created on 2022-09-20 14:29:20 **

** Found 8 DRC violations **
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(50,8000 mm, 127,0000 mm): Rect on Edge.Cuts
    @(85,8000 mm, 107,0000 mm): Arc on F.Silkscreen
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(50,8000 mm, 127,0000 mm): Rect on Edge.Cuts
    @(85,8000 mm, 107,0000 mm): Arc on F.Silkscreen
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(50,8000 mm, 127,0000 mm): Rect on Edge.Cuts
    @(89,2300 mm, 93,3500 mm): Line on F.Silkscreen
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(50,8000 mm, 127,0000 mm): Rect on Edge.Cuts
    @(89,2300 mm, 80,6500 mm): Line on F.Silkscreen
[silk_overlap]: Silkscreen overlap
    Rule: board setup constraints silk; Severity: warning
    @(82,5000 mm, 80,0000 mm): Arc on F.Silkscreen
    @(82,3700 mm, 93,3500 mm): Line on F.Silkscreen
[silk_overlap]: Silkscreen overlap
    Rule: board setup constraints silk; Severity: warning
    @(82,5000 mm, 70,0000 mm): Line on F.Silkscreen
    @(85,8000 mm, 67,0000 mm): Arc on F.Silkscreen
[silk_overlap]: Silkscreen overlap
    Rule: board setup constraints silk; Severity: warning
    @(81,5000 mm, 52,5000 mm): Line on F.Silkscreen
    @(81,3700 mm, 58,6500 mm): Line on F.Silkscreen
[silk_overlap]: Silkscreen overlap
    Rule: board setup constraints silk; Severity: warning
    @(81,5000 mm, 52,5000 mm): Line on F.Silkscreen
    @(81,3700 mm, 65,1900 mm): Line on F.Silkscreen

** Found 0 unconnected pads **

** Found 0 Footprint errors **

** End of Report **
