(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (title_block
    (title "ABS Simulator LEDs b")
    (date "2022-09-22")
    (rev "${version}")
    (company "WTF eg")
    (comment 1 "author: marble")
    (comment 2 "project id: 2022019")
  )

  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.2)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../production/gbr/")
    )
  )

  (property "version" "1.0")

  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 "Net-(D4-Pad1)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "+12V")

  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A) (tstamp 04d68e0d-550a-40cf-aace-2bfa5cbe0b8a)
    (at 149.93 85.25)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/9425f982-8fb5-4240-92cc-916be20d4139")
    (attr through_hole)
    (fp_text reference "D4" (at 6.27 0.04) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4cfd0ae0-7ef6-4113-8462-ab9612edfbfa)
    )
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9437025a-2471-4877-933c-394afbf90737)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.2)))
      (tstamp 6c7b66cf-5cc2-48d0-9b18-55822a29f853)
    )
    (fp_line (start -1.29 -1.545) (end -1.29 1.545) (layer "F.SilkS") (width 0.12) (tstamp f2a4df0b-6c30-40f0-a1fe-d679f5c482f0))
    (fp_arc (start 4.26 -0.000462) (mid 2.072002 2.880433) (end -1.29 1.54483) (layer "F.SilkS") (width 0.12) (tstamp 615ed0b5-762d-4244-b18a-c0a7781da0c1))
    (fp_arc (start -1.29 -1.54483) (mid 2.072002 -2.880433) (end 4.26 0.000462) (layer "F.SilkS") (width 0.12) (tstamp ea6eb121-4bef-42b5-b051-575b9df5de06))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 6c5e3bf5-23dc-4969-823d-a9edda8a337d))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp 211b1d7a-db36-4e15-9b75-2a42173c25aa))
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp 512fdeec-249e-4437-bf9a-6705cca2c63a))
    (fp_line (start -1.95 3.25) (end 4.5 3.25) (layer "F.CrtYd") (width 0.05) (tstamp 7c691cdf-d165-4ffe-b070-b037aac5ccbc))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25) (layer "F.CrtYd") (width 0.05) (tstamp baa76cc3-720f-4396-9f37-f5913a284c0c))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694) (layer "F.Fab") (width 0.1) (tstamp 77ab28f2-5ee1-46e8-acc2-2fd11a44c470))
    (fp_arc (start -1.23 -1.469694) (mid 4.17 0.000016) (end -1.230016 1.469666) (layer "F.Fab") (width 0.1) (tstamp 11d462d9-58ab-4ed4-bd82-23f676664603))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 12422e9e-8402-4744-807f-ec6aba2adc01))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 2d20c254-2369-4cfb-88f4-d1e35e2b5f4e))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive") (tstamp aed74ffd-7639-4f9e-9daf-c964b86b880c))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_4.5mm" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 099c66df-0106-4b79-a2b8-cb4eac457654)
    (at 100.1 95.75)
    (descr "Mounting Hole 4.5mm, no annular")
    (tags "mounting hole 4.5mm no annular")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/b9afa080-9a35-4a7b-8404-6df59773bff7")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -5.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2b06289f-f8ac-429b-b6b7-bb01c01f15b0)
    )
    (fp_text value "MountingHole" (at 0 5.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f30c14ac-b286-45e4-bd69-00f53ab3a422)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a65f4438-0a57-458d-ac12-634bfc8d18a0)
    )
    (fp_circle (center 0 0) (end 4.5 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 3f5c1d5a-9b10-4ba8-b6cc-205ec1baa4bc))
    (fp_circle (center 0 0) (end 4.75 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp c3209590-1b25-4e7b-9891-a7ace593644f))
    (pad "" np_thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.5) (layers *.Cu *.Mask) (tstamp bb9375f3-b9de-4aea-b1d9-067db56dd4bb))
  )

  (footprint "Connector_Wire:SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm" (layer "F.Cu")
    (tedit 5EB70B44) (tstamp 0a29d23d-f87c-45b6-87b3-8b0270b2a545)
    (at 145 84)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, reinforced insulation, conductor diameter 1.25mm, outer diameter 3.5mm, size source Multi-Contact FLEXI-xV 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/bf02469a-938c-4389-8039-6b9cc739de10")
    (attr exclude_from_pos_files)
    (fp_text reference "J5" (at 0 -2.95) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ce4ee471-7b65-42c1-b2cb-8c052820cb08)
    )
    (fp_text value "Conn_01x01" (at 0 2.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f6b9ceee-9cd1-45ca-ad33-bfa2831971e5)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.88 0.88) (thickness 0.13)))
      (tstamp 0ef45c92-11d3-4dc4-99c1-d67f1ed5ddc6)
    )
    (fp_line (start -2.5 -2.25) (end -2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp 510949bd-58ec-46e8-991a-abf652b1f392))
    (fp_line (start 2.5 -2.25) (end -2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 7ae77e14-b5fe-49f0-b90a-bc185f5fa90c))
    (fp_line (start -2.5 2.25) (end 2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp 91e72cff-8c9b-415b-84f7-411c2ba30875))
    (fp_line (start 2.5 2.25) (end 2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp ce845b90-1438-4371-90c0-720f4fc16323))
    (fp_circle (center 0 0) (end 1.75 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 7a776cd4-13c0-4d8f-8a64-620c39d3d99b))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.5 3.5) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.07142914286)
      (net 7 "Net-(D4-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 9b37883f-5214-45db-a8ac-62b373ad9ee7))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A) (tstamp 0fb98c73-6ec4-4251-9aa0-d6fdee418a56)
    (at 91.73 85.25)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/9fb431c6-dd5b-409c-9f68-9eeb23ca8992")
    (attr through_hole)
    (fp_text reference "D1" (at 6.27 0.04) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1924033e-df2b-40e0-973e-5ef07939249a)
    )
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 64256102-9e88-4a2c-a909-862360a090d7)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.2)))
      (tstamp cbefdb6e-3efc-47ad-8503-39d277b8a803)
    )
    (fp_line (start -1.29 -1.545) (end -1.29 1.545) (layer "F.SilkS") (width 0.12) (tstamp c6f730fd-e2ad-4ae8-86f8-ff6d811eb7c4))
    (fp_arc (start 4.26 -0.000462) (mid 2.072002 2.880433) (end -1.29 1.54483) (layer "F.SilkS") (width 0.12) (tstamp 4cfa62a9-7e30-4c64-882b-80e80e128f73))
    (fp_arc (start -1.29 -1.54483) (mid 2.072002 -2.880433) (end 4.26 0.000462) (layer "F.SilkS") (width 0.12) (tstamp 8174bbf6-0b90-48e4-9e72-cbb77b201655))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 95745125-9da1-4321-9d77-f7621ae6c789))
    (fp_line (start -1.95 3.25) (end 4.5 3.25) (layer "F.CrtYd") (width 0.05) (tstamp 1dd13529-d0dc-4493-b341-f03894d26049))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp 6febc297-4228-441f-89df-60d85a6cb3a7))
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp 8aaa9a92-117f-4884-bd1f-7de097b3c531))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25) (layer "F.CrtYd") (width 0.05) (tstamp b6217937-8fea-4e8b-951e-092e4b8cee71))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694) (layer "F.Fab") (width 0.1) (tstamp 9d62c8e3-5b0d-4e93-baca-7e6f7896f0c7))
    (fp_arc (start -1.23 -1.469694) (mid 4.17 0.000016) (end -1.230016 1.469666) (layer "F.Fab") (width 0.1) (tstamp f4f9e787-5441-46fa-8a44-2f8a7c8e28db))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp d1a14f4a-9bd5-4267-901d-1df6a61a1271))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 1fa8511a-43b5-425e-abb7-723b60b0a0fc))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 58e9b641-fd47-4b38-9e85-9b675b4d3e45))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 1d3e86e6-5de5-41e7-be27-cd6305f35867)
    (at 107 98 45)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/b7b95170-1828-49c5-ad6a-0ef6185ff351")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.37 45) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0034c6f6-5baa-4a50-bd19-00f23eb40acd)
    )
    (fp_text value "680" (at 5.08 2.370001 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9394bbbf-3592-468c-bb80-242d67fee7e1)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6413f003-bc33-487c-b4bd-35391ac6ec0c)
    )
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 0efce15e-e625-405e-b7ec-e6c6f7f238de))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 919c198e-7262-4114-ab22-f498b8bd7a0d))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp a6d3bf69-eec0-4f8b-9233-097755c089d2))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp d96d4d47-2742-47b9-8a3b-60e1b685cd77))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp ee5b897a-4728-43c1-835f-f4c13421d05d))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp faba4956-d19c-4df9-b3a2-881bd75c3eee))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 23440b38-b31c-48ad-bbb8-10334d65b3ad))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 460a1d42-2379-445a-b2fd-d61c90f3ae1e))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 676b2c50-5dc4-4052-8950-2bf7e429ed3c))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 8587f0a4-72fe-476a-ac9c-3f39e1e9065d))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 0bbe9ead-dadc-49e0-acbc-8efc65efd67e))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp 2a3fbbe8-bb01-467a-aa9e-67c69f7282b9))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp 34fc827a-e304-4034-b442-b7e4c98da1c6))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp a2e1dad8-c0fe-440b-89e8-6e1f62038679))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp e588620a-c170-4404-b2f6-b90378ecea80))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp f586aa21-190c-4418-8061-ba2dcf265a2f))
    (pad "1" thru_hole circle (at 0 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "+12V") (pintype "passive") (tstamp 3981ebba-12c4-4e08-bd18-4d308119c3ea))
    (pad "2" thru_hole oval (at 10.16 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)") (pintype "passive") (tstamp fa03a422-9afc-4655-bbe6-f96666cf1f7f))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 1fded854-0334-4a50-ae42-1898094d3f11)
    (at 126 98 45)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/7c6049c4-8563-4880-bb15-1fd8df8e9ed0")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 -2.37 45) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp ff63ef3c-ef00-413f-aaf0-a0c1a3fdfc37)
    )
    (fp_text value "680" (at 5.08 2.370001 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e8d498be-b072-448e-b2e0-f54c563dc666)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e0f2ba7d-0912-495c-90f8-db3d1940ea06)
    )
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 0229c3f8-7bc3-47d1-a0fc-fd4029ce5da9))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 07c46dbd-3c8f-4b6a-8406-8de97836e1ba))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 0ccb55f9-4d36-4649-bc8a-103e9b10ada5))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp 8401a42b-10f9-4d1c-8971-66a7abfd1ccb))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp ad788c7c-e8c8-410d-822d-351be0ef262f))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp d7cad7a0-f6c9-4dfa-ba31-5a8b9bb143ea))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 096c182d-c4e0-471b-868e-f4a5422d0eb1))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 4368b579-0776-422c-b8e9-3146b793e3a1))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 94d5643f-1790-4ed7-a718-97c1e457283e))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp c70db75f-4ff6-4e9c-aaab-aa34a64cd75d))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 507988e1-7504-4f9a-85d7-8dc37c22c79b))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp 6609240f-4b3b-4334-9694-e29a9e162d12))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 6a548cf0-92bb-4ff6-9f2c-52ce93a1eb46))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp 92085738-f7b2-4a7d-8f9d-3d96540172ba))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 9d02ffc0-9ad4-4a22-9a13-05342a209572))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp cff3698a-01a2-4a49-b4c6-5e8a48e6a0cc))
    (pad "1" thru_hole circle (at 0 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "+12V") (pintype "passive") (tstamp 596dd2f4-e400-46f7-aa67-0406588c738e))
    (pad "2" thru_hole oval (at 10.16 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad2)") (pintype "passive") (tstamp 9129bd50-c6c3-4544-abf2-1fff1c743ec2))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Wire:SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm" (layer "F.Cu")
    (tedit 5EB70B44) (tstamp 22c1b9ce-53fb-4de2-bbd5-e112ad2793a7)
    (at 83 97)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, reinforced insulation, conductor diameter 1.25mm, outer diameter 3.5mm, size source Multi-Contact FLEXI-xV 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/0647ef32-a44f-4db3-ba7a-eb742dac2490")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at 0 -2.95) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7f976c79-1535-4c55-9ab4-f6011e08f844)
    )
    (fp_text value "Conn_01x01" (at 0 2.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2ba21fce-c12b-40d4-b5e1-254a083e5abf)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.88 0.88) (thickness 0.13)))
      (tstamp 0c5d9fe6-099d-44a4-8dd9-d388aaf187b3)
    )
    (fp_line (start -2.5 2.25) (end 2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp 7cc84155-f4da-4ec6-8d66-3a35033a1718))
    (fp_line (start 2.5 -2.25) (end -2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 9b0737d8-8147-4c48-8226-bd0bd12614b1))
    (fp_line (start -2.5 -2.25) (end -2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp ae87188a-fa26-4b05-b0d7-fc74e84c7c79))
    (fp_line (start 2.5 2.25) (end 2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp aff6d495-a325-43df-b4fd-b12e780b7735))
    (fp_circle (center 0 0) (end 1.75 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp e561ec7a-b43c-4174-86d4-84b2d1325f36))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.5 3.5) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.07142914286)
      (net 9 "+12V") (pinfunction "Pin_1") (pintype "passive") (tstamp e79cea56-71bd-4f49-b249-b16aec42743a))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "MountingHole:MountingHole_4.5mm" (layer "F.Cu")
    (tedit 56D1B4CB) (tstamp 3bc90fc2-3c94-49a0-89ed-ffde9ab5784a)
    (at 144.1 95.75)
    (descr "Mounting Hole 4.5mm, no annular")
    (tags "mounting hole 4.5mm no annular")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/de237f06-e820-4082-b367-a32fa089b7a3")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -5.5) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 80975fee-7caa-473b-bb5a-64a9880e1883)
    )
    (fp_text value "MountingHole" (at 0 5.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f47cdbd-8bbc-40d7-b32b-0dd71ff40986)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2c5883ae-7c9d-4742-8e8b-41de4bd38458)
    )
    (fp_circle (center 0 0) (end 4.5 0) (layer "Cmts.User") (width 0.15) (fill none) (tstamp 09a46cb7-35ad-4fa0-b6ad-af2b2ebac4e7))
    (fp_circle (center 0 0) (end 4.75 0) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 30b2e605-fb2e-4279-ab5e-d3e7610eb844))
    (pad "" np_thru_hole circle (at 0 0) (size 4.5 4.5) (drill 4.5) (layers *.Cu *.Mask) (tstamp e2e113ff-d0e2-4365-8d4c-dfbc4db7d3e0))
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 5b3c6dc4-3097-4390-9fde-d320f9883274)
    (at 88 98 45)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/3af8b20b-3425-4389-ab0f-a7d4182ad103")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37 45) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4b8d2c10-d2d5-45be-899b-25b961c0f1c1)
    )
    (fp_text value "680" (at 5.08 2.370001 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4c6fe3c7-cd9b-43c9-b5f7-2a20fa7f956b)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 09570c4c-2dac-4176-b026-90525705b594)
    )
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp 41432817-a775-43c9-af96-13337bb397f2))
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp 648f6db8-1ffc-47e5-8c42-72239edd7104))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 6b8eb08d-9dd0-484c-b4dd-b2796a994941))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp a573da15-9dfa-4aed-a639-aa7713541d38))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp e4a66dbb-d487-41a6-a64b-185c7a059e57))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp f62392c8-86e7-48bd-b023-e1d9e748aab1))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 4417d9d9-5297-4fa9-b92b-92ef43525c4b))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 4c7f3ed5-e13f-45b2-9863-492fc3b12f1d))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp 5e48de36-a1b3-448a-8960-9c7af1d5c090))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp f0d0b94c-ebb0-46c7-97cc-b93134363a00))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 2e72d2b6-0b50-430b-950d-d70888ebda72))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 35b4a7c8-c73a-4eda-857e-afb77568fc6b))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp 4b595f8f-0616-4047-8959-a9ce31ea7daf))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp 82d1dbcc-9187-44f3-8251-3e8dd726f73f))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 9ddd40e8-482f-4604-baa2-a61922d06e33))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp c89878f4-8f3e-4569-beeb-9723b0378ac9))
    (pad "1" thru_hole circle (at 0 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "+12V") (pintype "passive") (tstamp 4015a916-5c30-4cc1-b542-3853b69f692b))
    (pad "2" thru_hole oval (at 10.16 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)") (pintype "passive") (tstamp 350b7875-5d0d-40b5-af1f-0aeb359bc46e))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B) (tstamp 62493665-0339-49f2-bf40-b0d7cf08697b)
    (at 151 98 45)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/23eccad2-a18c-43fd-9d24-1fd9a8e1f618")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 -2.37 45) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7e63588c-c2fd-493f-9fe3-bc1b851c6cd1)
    )
    (fp_text value "680" (at 5.08 2.370001 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7d27b3e2-0956-430c-982b-e17e0a85e479)
    )
    (fp_text user "${REFERENCE}" (at 5.08 0 45) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 76d7dea5-6c73-4685-bd93-5a36a7ffc07f)
    )
    (fp_line (start 1.04 0) (end 1.81 0) (layer "F.SilkS") (width 0.12) (tstamp 0c7b8086-3835-4eb0-8adb-21a269d0c531))
    (fp_line (start 1.81 -1.37) (end 1.81 1.37) (layer "F.SilkS") (width 0.12) (tstamp 439d1dd2-8520-4272-8fc6-167055b36e3f))
    (fp_line (start 8.35 -1.37) (end 1.81 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 46df3f87-64cb-4ae6-b588-cb109a80790f))
    (fp_line (start 1.81 1.37) (end 8.35 1.37) (layer "F.SilkS") (width 0.12) (tstamp 8d5673f8-3815-4399-9d69-75eda3895539))
    (fp_line (start 8.35 1.37) (end 8.35 -1.37) (layer "F.SilkS") (width 0.12) (tstamp 96559978-2d0d-4816-a73a-d370c4f64659))
    (fp_line (start 9.12 0) (end 8.35 0) (layer "F.SilkS") (width 0.12) (tstamp bb8ad497-80e0-4e31-a6cc-025edeec2f68))
    (fp_line (start -1.05 1.5) (end 11.21 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 20c32f99-8d8b-4806-ac53-0438730a9613))
    (fp_line (start -1.05 -1.5) (end -1.05 1.5) (layer "F.CrtYd") (width 0.05) (tstamp 87beb32b-6f71-4ceb-9f1b-007d65985a3a))
    (fp_line (start 11.21 -1.5) (end -1.05 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp c88523bd-efd6-4a97-b282-c160e8b63e50))
    (fp_line (start 11.21 1.5) (end 11.21 -1.5) (layer "F.CrtYd") (width 0.05) (tstamp d72d951a-4fba-4230-b308-662947c552fd))
    (fp_line (start 0 0) (end 1.93 0) (layer "F.Fab") (width 0.1) (tstamp 32fee519-29ba-4048-98b9-bcb11e7cc1ec))
    (fp_line (start 1.93 -1.25) (end 1.93 1.25) (layer "F.Fab") (width 0.1) (tstamp 8afae9a8-2f95-4af7-a07f-7b3037821d4c))
    (fp_line (start 1.93 1.25) (end 8.23 1.25) (layer "F.Fab") (width 0.1) (tstamp 954e0b96-4ff6-4542-8c49-9d0a3ecd70a5))
    (fp_line (start 8.23 1.25) (end 8.23 -1.25) (layer "F.Fab") (width 0.1) (tstamp 9e3c1143-17f1-44b6-bcb7-c9b939887af7))
    (fp_line (start 10.16 0) (end 8.23 0) (layer "F.Fab") (width 0.1) (tstamp da9e17e7-fcd7-4f3a-bff4-e8366026db0d))
    (fp_line (start 8.23 -1.25) (end 1.93 -1.25) (layer "F.Fab") (width 0.1) (tstamp f64654f4-4d2c-472e-9cc1-75070a6f0ad6))
    (pad "1" thru_hole circle (at 0 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "+12V") (pintype "passive") (tstamp 65271a87-bad6-4dd7-80d7-ef3c8c20fd9f))
    (pad "2" thru_hole oval (at 10.16 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)") (pintype "passive") (tstamp f49971c1-3c20-453c-9366-9ccb6eda23d2))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Wire:SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm" (layer "F.Cu")
    (tedit 5EB70B44) (tstamp 6dde5481-e904-4353-8897-a7d717785d21)
    (at 87 84)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, reinforced insulation, conductor diameter 1.25mm, outer diameter 3.5mm, size source Multi-Contact FLEXI-xV 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/a9921d4f-98ee-4d23-bb6b-c7b615bc538c")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at 0 -2.95) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 94093c58-d36f-4e7b-a4ae-4f362e9b2e7c)
    )
    (fp_text value "Conn_01x01" (at 0 2.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7111c7de-c87a-4287-a5af-f1a486574e02)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.88 0.88) (thickness 0.13)))
      (tstamp 4e424106-44ce-4289-937d-98a1b87e011a)
    )
    (fp_line (start 2.5 2.25) (end 2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 63d3d6bd-454a-4085-b430-acbcfee09408))
    (fp_line (start 2.5 -2.25) (end -2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp ba52e4eb-e837-489f-a5cc-8cea3793c1ac))
    (fp_line (start -2.5 -2.25) (end -2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp bf482642-1352-46c6-8833-d9d142cb2e88))
    (fp_line (start -2.5 2.25) (end 2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp d18c65aa-9c1a-4e2b-a832-c096e8c0237f))
    (fp_circle (center 0 0) (end 1.75 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 39bcc12e-c482-4e8c-bbd5-cade521ab0df))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.5 3.5) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.07142914286)
      (net 1 "Net-(D1-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 5a3344e7-2663-40b7-a127-4aa8a953e023))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A) (tstamp a91889b8-bb63-4734-b1a0-2da98c6d9412)
    (at 130.525 85.25)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/ea1f45bd-7272-4a52-bc07-a787b1bb8422")
    (attr through_hole)
    (fp_text reference "D3" (at 6.27 0.04) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8e16e5fe-0ab8-4660-a240-fbcc4c3a3584)
    )
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b0ba3052-115b-4ffe-8b35-7ff907e90137)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.2)))
      (tstamp e2e50232-1a87-450c-b076-ee90b68607b7)
    )
    (fp_line (start -1.29 -1.545) (end -1.29 1.545) (layer "F.SilkS") (width 0.12) (tstamp 1ce0473c-6233-4f6d-ab50-169d5c3faa1b))
    (fp_arc (start 4.26 -0.000462) (mid 2.072002 2.880433) (end -1.29 1.54483) (layer "F.SilkS") (width 0.12) (tstamp 29d4c810-3d26-4aac-99ea-cc8ba21011de))
    (fp_arc (start -1.29 -1.54483) (mid 2.072002 -2.880433) (end 4.26 0.000462) (layer "F.SilkS") (width 0.12) (tstamp 45a8a7a4-9c17-42e7-858b-22f6bd11c791))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 92a52816-cc03-4dd6-b4a6-905017bf687b))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25) (layer "F.CrtYd") (width 0.05) (tstamp 4e42622b-88eb-4b76-8d78-a08f0306a5ac))
    (fp_line (start -1.95 3.25) (end 4.5 3.25) (layer "F.CrtYd") (width 0.05) (tstamp a9bb875d-9536-4806-9895-8dd6633708d5))
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp fbcfd2ea-382a-43e0-850e-2dd2593979a2))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp fd7f201d-04d8-44c0-8e59-c5915b483524))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694) (layer "F.Fab") (width 0.1) (tstamp f1471c4c-0c28-4030-af8a-9cb29ccbbf72))
    (fp_arc (start -1.23 -1.469694) (mid 4.17 0.000016) (end -1.230016 1.469666) (layer "F.Fab") (width 0.1) (tstamp 7a9786a4-eb04-4d87-8a3d-4b30c8ba9cf6))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 14582179-d588-4568-9657-9643ad4fc434))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive") (tstamp 2ad7881e-3a18-46cc-a0b2-ed569eb07bbf))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 9627a0a3-84e0-4fa1-a66b-26ad4e1c96ea))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Wire:SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm" (layer "F.Cu")
    (tedit 5EB70B44) (tstamp de9a402b-e367-4579-90ca-feaa36552e64)
    (at 126 84)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, reinforced insulation, conductor diameter 1.25mm, outer diameter 3.5mm, size source Multi-Contact FLEXI-xV 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/5e261ca5-26a2-473f-a32c-848b4080cc5d")
    (attr exclude_from_pos_files)
    (fp_text reference "J4" (at 0 -2.95) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9678aa85-6cc5-4694-b028-8cf16de1b26d)
    )
    (fp_text value "Conn_01x01" (at 0 2.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0ea5c215-7ca9-4dd9-b158-ffde7aea8f0c)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.88 0.88) (thickness 0.13)))
      (tstamp c47c57ff-855d-474b-8f3e-91146149b116)
    )
    (fp_line (start 2.5 2.25) (end 2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 09cc6593-e8dd-4e8b-ba71-4aac6ff4e416))
    (fp_line (start -2.5 -2.25) (end -2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp 190482a2-c78c-4ebf-91b8-7dfe4c9a132b))
    (fp_line (start 2.5 -2.25) (end -2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 2983a162-8c0e-4e5f-87d7-9b333243eb04))
    (fp_line (start -2.5 2.25) (end 2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp c0a00878-ca82-4e4b-b26b-545d70072ccf))
    (fp_circle (center 0 0) (end 1.75 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 95505733-1d77-45b0-9fd2-d080a31cb2bd))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.5 3.5) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.07142914286)
      (net 5 "Net-(D3-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp 342a020c-91f6-4003-abc8-e413a4e75f82))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tedit 5995936A) (tstamp e09c1095-ef96-4da2-a45e-7c303f86d57f)
    (at 111.125 85.25)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/cb404871-ccd1-4901-8766-cd99a61569da")
    (attr through_hole)
    (fp_text reference "D2" (at 6.27 0.04) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b51af8d0-62b8-4044-b393-fe8401ea11a2)
    )
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 37bf9a8c-0c61-4268-a21f-7e7700ef4fe5)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
      (effects (font (size 0.8 0.8) (thickness 0.2)))
      (tstamp d9713a8a-154a-4a2d-b2e3-80b262a19242)
    )
    (fp_line (start -1.29 -1.545) (end -1.29 1.545) (layer "F.SilkS") (width 0.12) (tstamp aae8bbd7-2d5f-4e81-aa58-1ec298924f47))
    (fp_arc (start 4.26 -0.000462) (mid 2.072002 2.880433) (end -1.29 1.54483) (layer "F.SilkS") (width 0.12) (tstamp b8b622fd-f9ff-4409-9c6a-b41edbe2fd68))
    (fp_arc (start -1.29 -1.54483) (mid 2.072002 -2.880433) (end 4.26 0.000462) (layer "F.SilkS") (width 0.12) (tstamp ca7e1bc6-f69f-41bc-9417-c0eb641e8c20))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp a5057d75-0896-4a7f-bae3-dcc6b7b94629))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp 82b03c18-9cbb-4d4c-8220-87a7afb66a95))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25) (layer "F.CrtYd") (width 0.05) (tstamp 9585efae-9fe6-4e27-a3de-4243cf3fd79f))
    (fp_line (start -1.95 3.25) (end 4.5 3.25) (layer "F.CrtYd") (width 0.05) (tstamp f053103d-aa7e-42d9-b033-c59af29c73fa))
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25) (layer "F.CrtYd") (width 0.05) (tstamp f77f817b-6846-4fd7-a9b7-5a2f1b19057c))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694) (layer "F.Fab") (width 0.1) (tstamp 543cb631-cc41-4917-b103-189a13817497))
    (fp_arc (start -1.23 -1.469694) (mid 4.17 0.000016) (end -1.230016 1.469666) (layer "F.Fab") (width 0.1) (tstamp f7178c48-8df9-4a51-baee-5633ecfe689c))
    (fp_circle (center 1.27 0) (end 3.77 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 23c9f83a-80c7-417c-a07a-8460d7570d90))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive") (tstamp b44cd140-c890-4d82-893e-dbad8300c234))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive") (tstamp 2c4a965e-c976-4cf3-8226-ef1dfdb23584))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_Wire:SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm" (layer "F.Cu")
    (tedit 5EB70B44) (tstamp e7fa6b35-c77c-4a0d-b64d-35a4dd1c00a5)
    (at 106 84)
    (descr "Soldered wire connection, for a single 0.75 mm² wire, reinforced insulation, conductor diameter 1.25mm, outer diameter 3.5mm, size source Multi-Contact FLEXI-xV 0.75 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.75sqmm")
    (property "Sheetfile" "ABS_Simulator_LEDs_b.kicad_sch")
    (property "Sheetname" "")
    (path "/dceb8dc1-e087-4f96-b6b5-d615692d2b53")
    (attr exclude_from_pos_files)
    (fp_text reference "J3" (at 0 -2.95) (layer "F.SilkS") hide
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7054ca20-4679-4fad-a73d-3d3a49848a9c)
    )
    (fp_text value "Conn_01x01" (at 0 2.95) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 48832a50-3ea4-40d5-9309-fb0fe630c5e0)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.88 0.88) (thickness 0.13)))
      (tstamp c1001481-d021-4a99-ad37-3465f7ed2b10)
    )
    (fp_line (start -2.5 -2.25) (end -2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp 3f26af07-ec71-4773-bf17-2e912e7d6af7))
    (fp_line (start 2.5 -2.25) (end -2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp 455a5fd6-ac33-439d-8619-128942525e1e))
    (fp_line (start 2.5 2.25) (end 2.5 -2.25) (layer "F.CrtYd") (width 0.05) (tstamp a19e6ddd-6343-4843-ba9a-ddcecb7d40f2))
    (fp_line (start -2.5 2.25) (end 2.5 2.25) (layer "F.CrtYd") (width 0.05) (tstamp da9d5d65-28bb-4970-bbc0-ff4ab42df508))
    (fp_circle (center 0 0) (end 1.75 0) (layer "F.Fab") (width 0.1) (fill none) (tstamp 8a2f0e7b-b5a2-42f4-877d-182502aa766d))
    (pad "1" thru_hole roundrect (at 0 0) (size 3.5 3.5) (drill 1.55) (layers *.Cu *.Mask) (roundrect_rratio 0.07142914286)
      (net 3 "Net-(D2-Pad1)") (pinfunction "Pin_1") (pintype "passive") (tstamp e34634b9-0069-4c9c-89b8-538bc3865164))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.75sqmm_1x01_D1.25mm_OD3.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 160.000001 100) (end 160.000001 80.999999) (layer "Dwgs.User") (width 0.2) (tstamp 15597100-861d-4327-b4de-729766846be8))
  (gr_line (start 80 100) (end 80 80.999999) (layer "Dwgs.User") (width 0.2) (tstamp 18169fe0-476b-40fd-8d2b-ac05be9e78fe))
  (gr_circle (center 100.1 95.75) (end 102.35 95.75) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 3c517e5b-4d56-4da0-a3df-8b2faf958111))
  (gr_line (start 160.000001 80.999999) (end 80 80.999999) (layer "Dwgs.User") (width 0.2) (tstamp 3e0e2dc1-d753-4358-b458-8c71f26df2b4))
  (gr_line (start 160.000001 100) (end 80 100) (layer "Dwgs.User") (width 0.2) (tstamp 4e3feddf-d470-4321-8560-a9d2747868c6))
  (gr_circle (center 151.2 85.25) (end 153.75 85.25) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 6356e238-bf56-416c-b30a-ec68fc4cae2e))
  (gr_circle (center 93 85.25) (end 95.55 85.25) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 6415aace-eb9c-4daa-85ed-87b73251c599))
  (gr_circle (center 144.1 95.75) (end 146.35 95.75) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 897057eb-22f1-4b0e-a9a7-bcbd627a8d56))
  (gr_circle (center 131.8 85.25) (end 134.35 85.25) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp 9f414c47-0689-4da5-b28a-f11ba8b626af))
  (gr_circle (center 112.4 85.25) (end 114.95 85.25) (layer "Dwgs.User") (width 0.2) (fill none) (tstamp dafcf077-0c5f-4148-8bb1-311b5a104237))
  (gr_rect (start 80 100) (end 160 81) (layer "Edge.Cuts") (width 0.1) (fill none) (tstamp 9131a02e-7324-413a-8c04-4be4cda290a1))
  (gr_text "2" (at 106.000011 87.969677) (layer "B.SilkS") (tstamp 29e67471-f8f2-4bb5-a174-242e5a0bb518)
    (effects (font (size 2 2) (thickness 0.4)) (justify mirror))
  )
  (gr_text "3" (at 125.961719 87.9348) (layer "B.SilkS") (tstamp 56ad4d79-77b5-429b-b837-4f5ed1d3f010)
    (effects (font (size 2 2) (thickness 0.4)) (justify mirror))
  )
  (gr_text "1" (at 86.984425 87.965123) (layer "B.SilkS") (tstamp 9668b879-1f43-4c7b-9ac7-b99ec4c056c1)
    (effects (font (size 2 2) (thickness 0.4)) (justify mirror))
  )
  (gr_text "+12V" (at 85 93) (layer "B.SilkS") (tstamp b0def86d-cb3f-4042-9a91-1d4aa5653b32)
    (effects (font (size 2 2) (thickness 0.4)) (justify mirror))
  )
  (gr_text "4" (at 144.980639 87.949818) (layer "B.SilkS") (tstamp e022fbdd-deca-409c-9600-03bde93e5343)
    (effects (font (size 2 2) (thickness 0.4)) (justify mirror))
  )
  (gr_text "1" (at 87 88) (layer "F.SilkS") (tstamp 03db06e4-d29c-418d-a971-1e04ad69a34e)
    (effects (font (size 2 2) (thickness 0.4)))
  )
  (gr_text "3" (at 125.999989 87.969677) (layer "F.SilkS") (tstamp 12c5914c-6fd9-4a73-8748-b169f7bdbcb2)
    (effects (font (size 2 2) (thickness 0.4)))
  )
  (gr_text "2" (at 105.999989 87.969677) (layer "F.SilkS") (tstamp 14b468e4-bb5e-4e57-a3d0-7bcf8fa76af3)
    (effects (font (size 2 2) (thickness 0.4)))
  )
  (gr_text "+12V" (at 84 93) (layer "F.SilkS") (tstamp 5ec0d98f-7ca4-4318-97b9-95bcc2c99e25)
    (effects (font (size 2 2) (thickness 0.4)))
  )
  (gr_text "v${version}" (at 159 98) (layer "F.SilkS") (tstamp 6bdf6547-e420-4aef-bf78-1111a9dbd5d2)
    (effects (font (size 1 1) (thickness 0.15)) (justify right))
  )
  (gr_text "4" (at 145.019361 87.949818) (layer "F.SilkS") (tstamp ac4f4054-b110-49db-9a2c-c83cad7d78b7)
    (effects (font (size 2 2) (thickness 0.4)))
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp 0906a23a-1093-4e2b-aef9-729ea45e7da2)
    (pts (xy 93 85.25) (xy 112.4 85.25))
    (height -6.25)
    (orientation 0)
    (gr_text "19,4000 mm" (at 102.7 77.85) (layer "User.1") (tstamp 0906a23a-1093-4e2b-aef9-729ea45e7da2)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp 0950e88a-5c65-41ff-a175-556c1a1e7ac5)
    (pts (xy 80 100) (xy 100.1 95.75))
    (height 3)
    (orientation 0)
    (gr_text "20,1000 mm" (at 90.05 101.85) (layer "User.1") (tstamp 0950e88a-5c65-41ff-a175-556c1a1e7ac5)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp 20e10f3a-0111-4e61-92dc-7a254eab1807)
    (pts (xy 80 80.999999) (xy 160.000001 80.999999))
    (height -10.999999)
    (orientation 0)
    (gr_text "80,0000 mm" (at 120 68.85) (layer "User.1") (tstamp 20e10f3a-0111-4e61-92dc-7a254eab1807)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp 222cb88b-a14c-44e9-86d7-a04794437f49)
    (pts (xy 100.1 95.75) (xy 144.1 95.75))
    (height 7.25)
    (orientation 0)
    (gr_text "44,0000 mm" (at 122.1 101.85) (layer "User.1") (tstamp 222cb88b-a14c-44e9-86d7-a04794437f49)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp 54e01b89-912b-4e25-af5a-ab96bd656484)
    (pts (xy 112.4 85.25) (xy 131.8 85.25))
    (height -6.25)
    (orientation 0)
    (gr_text "19,4000 mm" (at 122.1 77.85) (layer "User.1") (tstamp 54e01b89-912b-4e25-af5a-ab96bd656484)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp 823bb41a-0b52-42ca-b4cc-714a576df849)
    (pts (xy 131.8 85.25) (xy 151.2 85.25))
    (height -6.25)
    (orientation 0)
    (gr_text "19,4000 mm" (at 141.5 77.85) (layer "User.1") (tstamp 823bb41a-0b52-42ca-b4cc-714a576df849)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp ac4c4d2c-b620-4184-8587-7608103c04bc)
    (pts (xy 80 100) (xy 100.1 95.75))
    (height -2)
    (orientation 1)
    (gr_text "4,2500 mm" (at 76.85 97.875 90) (layer "User.1") (tstamp ac4c4d2c-b620-4184-8587-7608103c04bc)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp c3a5d6ad-02f2-4244-aa10-8da990dc024f)
    (pts (xy 80 80.999999) (xy 93 85.25))
    (height -1.999999)
    (orientation 0)
    (gr_text "13,0000 mm" (at 86.5 77.85) (layer "User.1") (tstamp c3a5d6ad-02f2-4244-aa10-8da990dc024f)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp ccfe4071-869d-4adc-be4d-271a7327cd1c)
    (pts (xy 80 100) (xy 80 80.999999))
    (height -10)
    (orientation 1)
    (gr_text "19,0000 mm" (at 68.85 90.5 90) (layer "User.1") (tstamp ccfe4071-869d-4adc-be4d-271a7327cd1c)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "User.1") (tstamp dc7b5d40-ffc6-4081-b74e-09e06ccb6e98)
    (pts (xy 80 100) (xy 93 85.25))
    (height -5)
    (orientation 1)
    (gr_text "14,7500 mm" (at 73.85 92.625 90) (layer "User.1") (tstamp dc7b5d40-ffc6-4081-b74e-09e06ccb6e98)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )

  (segment (start 91.73 85.25) (end 90.48 84) (width 1) (layer "B.Cu") (net 1) (tstamp bb206b3d-1e4c-4347-aaa5-fcd8c6faddb4))
  (segment (start 90.48 84) (end 87 84) (width 1) (layer "B.Cu") (net 1) (tstamp e9e50944-5529-4408-ac66-20b47be0cea4))
  (segment (start 94.27 87.27) (end 95.184205 88.184205) (width 1) (layer "B.Cu") (net 2) (tstamp 0e9df740-bdb2-4bed-8300-686282be0bad))
  (segment (start 94.27 85.25) (end 94.27 87.27) (width 1) (layer "B.Cu") (net 2) (tstamp 4b100331-2f0c-4de3-9a3e-cc7a54724606))
  (segment (start 95.184205 90.815795) (end 95.184205 88.184205) (width 1) (layer "B.Cu") (net 2) (tstamp f5d791b0-d10c-4d0a-9752-6c451d59ffe3))
  (segment (start 109.875 84) (end 106 84) (width 1) (layer "B.Cu") (net 3) (tstamp 7069acd7-7ada-4077-98f5-874c946f5a3a))
  (segment (start 111.125 85.25) (end 109.875 84) (width 1) (layer "B.Cu") (net 3) (tstamp 82948ac3-2e78-49fe-9d15-1584944d43ea))
  (segment (start 113.665 87.665) (end 114.184205 88.184205) (width 1) (layer "B.Cu") (net 4) (tstamp 0f99998b-3332-46d0-b61c-d5ffdc9a1e3e))
  (segment (start 113.665 85.25) (end 113.665 87.665) (width 1) (layer "B.Cu") (net 4) (tstamp 1ce48bc0-a3a1-49e9-b94b-27d9ad1d0c86))
  (segment (start 114.184205 90.815795) (end 114.184205 88.184205) (width 1) (layer "B.Cu") (net 4) (tstamp cf9c2275-5a2d-48c1-b923-7fda593d585b))
  (segment (start 130.525 85.25) (end 129.275 84) (width 1) (layer "B.Cu") (net 5) (tstamp 9c953cf2-04df-42e9-93b8-1de1d7960d51))
  (segment (start 129.275 84) (end 126 84) (width 1) (layer "B.Cu") (net 5) (tstamp f60215dd-d9ab-4c0b-9c9e-d278b698fa20))
  (segment (start 133.184205 90.815795) (end 133.184205 85.369205) (width 1) (layer "B.Cu") (net 6) (tstamp 7822e2a9-03a1-4d0e-95dd-99308b0ee8a2))
  (segment (start 133.184205 85.369205) (end 133.065 85.25) (width 1) (layer "B.Cu") (net 6) (tstamp 85565643-157c-4103-a5eb-ca874e244605))
  (segment (start 148.68 84) (end 145 84) (width 1) (layer "B.Cu") (net 7) (tstamp 64cc5eef-36fe-4d4f-b648-f9eea54e5d96))
  (segment (start 149.93 85.25) (end 148.68 84) (width 1) (layer "B.Cu") (net 7) (tstamp 7cc63374-4ebb-405d-81f9-ad4569ae1b92))
  (segment (start 152.61841 85.25) (end 152.47 85.25) (width 1) (layer "B.Cu") (net 8) (tstamp 31caf699-d898-456f-942c-b938d08b3340))
  (segment (start 158.184205 90.815795) (end 152.61841 85.25) (width 1) (layer "B.Cu") (net 8) (tstamp 8cf873c4-c20d-412a-8351-64ed0f351443))
  (segment (start 150 99) (end 151 98) (width 1) (layer "B.Cu") (net 9) (tstamp 19b7e47b-fae7-4ce4-8e8e-2adfcc86063c))
  (segment (start 83 97) (end 87 97) (width 1) (layer "B.Cu") (net 9) (tstamp 462f5f57-1674-4b14-8ac7-b1afc29319fd))
  (segment (start 89 99) (end 106 99) (width 1) (layer "B.Cu") (net 9) (tstamp 4a328598-2a93-48c6-a2c0-f29b91d23994))
  (segment (start 137 98) (end 138 99) (width 1) (layer "B.Cu") (net 9) (tstamp 95934133-1ea7-43b1-9590-78448415bbf1))
  (segment (start 126 98) (end 137 98) (width 1) (layer "B.Cu") (net 9) (tstamp 96c039e5-c756-47db-9110-c70dfa09e1c8))
  (segment (start 88 98) (end 89 99) (width 1) (layer "B.Cu") (net 9) (tstamp 9ddaff87-6ba1-48c3-bed3-c693b295f6d4))
  (segment (start 138 99) (end 150 99) (width 1) (layer "B.Cu") (net 9) (tstamp ab84945b-1539-4f93-8289-f1bec4581847))
  (segment (start 106 99) (end 107 98) (width 1) (layer "B.Cu") (net 9) (tstamp b4cd69d1-d87e-432a-8128-fbbe3ba2fc18))
  (segment (start 87 97) (end 88 98) (width 1) (layer "B.Cu") (net 9) (tstamp b6415bba-2f69-4928-92ee-6655c7847baf))
  (segment (start 107 98) (end 126 98) (width 1) (layer "B.Cu") (net 9) (tstamp c8ad0f9c-1a64-4731-9a42-5b3d7fc45691))

  (group "" (id a4a915ee-e4d0-4810-b31d-6113fec96cd4)
    (members
      15597100-861d-4327-b4de-729766846be8
      18169fe0-476b-40fd-8d2b-ac05be9e78fe
      3c517e5b-4d56-4da0-a3df-8b2faf958111
      3e0e2dc1-d753-4358-b458-8c71f26df2b4
      4e3feddf-d470-4321-8560-a9d2747868c6
      6356e238-bf56-416c-b30a-ec68fc4cae2e
      6415aace-eb9c-4daa-85ed-87b73251c599
      897057eb-22f1-4b0e-a9a7-bcbd627a8d56
      9f414c47-0689-4da5-b28a-f11ba8b626af
      dafcf077-0c5f-4148-8bb1-311b5a104237
    )
  )
)
