** Drc report for /home/marble/wtf/2022019/Alternator_Motor_Driver/source/Alternator_Motor_Driver.kicad_pcb **
** Created on 2022-09-23 17:47:25 **

** Found 27 DRC violations **
[courtyards_overlap]: Courtyards overlap
    Local override; Severity: error
    @(160,0200 mm, 81,2800 mm): Footprint H3
    @(157,4800 mm, 86,3600 mm): Footprint Q3
[courtyards_overlap]: Courtyards overlap
    Local override; Severity: error
    @(144,7800 mm, 81,2800 mm): Footprint H2
    @(142,2400 mm, 86,3600 mm): Footprint Q2
[courtyards_overlap]: Courtyards overlap
    Local override; Severity: error
    @(127,0000 mm, 86,3600 mm): Footprint Q1
    @(129,5400 mm, 81,2800 mm): Footprint H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(158,1700 mm, 83,0900 mm): Line on F.Silkscreen
    @(160,0200 mm, 81,2800 mm): Through hole pad 1 [W] of H3
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(158,1700 mm, 83,0900 mm): Line on F.Silkscreen
    @(158,1638 mm, 83,1362 mm): Through hole pad 1 [W] of H3
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(139,6600 mm, 84,6000 mm): Line on F.Silkscreen
    @(144,7800 mm, 81,2800 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(139,6600 mm, 83,0900 mm): Line on F.Silkscreen
    @(144,7800 mm, 81,2800 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(139,6600 mm, 83,0900 mm): Line on F.Silkscreen
    @(142,9238 mm, 83,1362 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(139,6600 mm, 83,0900 mm): Line on F.Silkscreen
    @(146,6362 mm, 83,1362 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(142,9300 mm, 83,0900 mm): Line on F.Silkscreen
    @(144,7800 mm, 81,2800 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(142,9300 mm, 83,0900 mm): Line on F.Silkscreen
    @(142,9238 mm, 83,1362 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(146,6310 mm, 83,0900 mm): Line on F.Silkscreen
    @(144,7800 mm, 81,2800 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(146,6310 mm, 83,0900 mm): Line on F.Silkscreen
    @(146,6362 mm, 83,1362 mm): Through hole pad 1 [V] of H2
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(124,4200 mm, 84,6000 mm): Line on F.Silkscreen
    @(129,5400 mm, 81,2800 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(127,6900 mm, 83,0900 mm): Line on F.Silkscreen
    @(129,5400 mm, 81,2800 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(127,6900 mm, 83,0900 mm): Line on F.Silkscreen
    @(127,6838 mm, 83,1362 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(131,3910 mm, 83,0900 mm): Line on F.Silkscreen
    @(129,5400 mm, 81,2800 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(131,3910 mm, 83,0900 mm): Line on F.Silkscreen
    @(131,3962 mm, 83,1362 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(124,4200 mm, 83,0900 mm): Line on F.Silkscreen
    @(129,5400 mm, 81,2800 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(124,4200 mm, 83,0900 mm): Line on F.Silkscreen
    @(127,6838 mm, 83,1362 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(124,4200 mm, 83,0900 mm): Line on F.Silkscreen
    @(131,3962 mm, 83,1362 mm): Through hole pad 1 [U] of H1
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(154,9000 mm, 83,0900 mm): Line on F.Silkscreen
    @(161,8762 mm, 83,1362 mm): Through hole pad 1 [W] of H3
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(154,9000 mm, 83,0900 mm): Line on F.Silkscreen
    @(160,0200 mm, 81,2800 mm): Through hole pad 1 [W] of H3
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(154,9000 mm, 83,0900 mm): Line on F.Silkscreen
    @(158,1638 mm, 83,1362 mm): Through hole pad 1 [W] of H3
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(154,9000 mm, 84,6000 mm): Line on F.Silkscreen
    @(160,0200 mm, 81,2800 mm): Through hole pad 1 [W] of H3
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(161,8710 mm, 83,0900 mm): Line on F.Silkscreen
    @(161,8762 mm, 83,1362 mm): Through hole pad 1 [W] of H3
[silk_over_copper]: Silkscreen clipped by solder mask
    Rule: board setup constraints silk; Severity: warning
    @(161,8710 mm, 83,0900 mm): Line on F.Silkscreen
    @(160,0200 mm, 81,2800 mm): Through hole pad 1 [W] of H3

** Found 0 unconnected pads **

** Found 0 Footprint errors **

** End of Report **
